Joey Krotz

Met 321

3/28/11

Power Hungry

Chapter 12:

1. When the wind wasn’t blowing in January of 2009 eastern Washington and Oregon used Hydropower to compensate for the lack of wind power.
2. The best backup for wind power plants is to use natural gas facilities.
	1. Solar power facilities
	2. Hydro power facilities
	3. Natural gas facilities
	4. Coal plants
3. Natural gas facilities only need to be manned 24 hours a day to back up wind power plants.
	1. 8
	2. 12
	3. 16
	4. 24